1st Re-issue
DATA
Vacuum/Hydraulic system
System 	Split hydraulic system with vacuum assistance meeting EEC regulations. See 'Description'.

Actuation	Service - footbrake vacuum hydraulic to all wheels. A load sensing valve controls rear brake application.
Secondary - footbrake vacuum hydraulic to unfailed half of system. Parking - handbrake through mechanical linkage to rear brakes only.

Brake Assemblies 	Front and rear drum brakes are self adjusting with manual override (de-adjust) facility.
Make	Front	Rear	
	Girling	Girling	
Type	H LS/S	Duo Servo	
Linings - make	RB35 - Ferodo 2629 others - Mintex S4	All - Mintex S2/S3	
- diameter	RB35 - 282,4 (111)		
	others - 330,2 (13)	All - 307,8 (120	
- width	All - 76,2 (3)	RB66 - 101,6 (4) others - 76,2 (3)	
- thickness	RB35 - 5,8 (0.23)		
	others - 9,7 (0.38)	All - 7,6 (0.30)	
Wheel cylinders - No. per wheel	2	1	
- Diameter	31,8 (1.25)	RB35 - 22,2 (0.875) others 25,4 (1.0)	
All dimensions in millimetres (inches) Master Cylinder

Make 	Girling with integral fluid reservoir and fluid level indicator.

Diameter 	27 mm (1.062 in)

Stroke 	34,5 mm (1.358 in)

© Talbot Motor Company Ltd 1980
I
W.S.M. 3005