CHASSIS No. 219001	BRAKES

FRONT	S75 P.S.V.
make 	Girling
type 	2 leading shoe drum H.L.S.S. manual adjust
size 	330 x 127 (13" x 5")
wheel cylinder 	31,75 (1.25") dia.
lining material 	Don 242

REAR	S75 Haulage
make 	Lockheed
type 	duo-servo drum - auto. adjust
size 	300 x 140 (13" x 5.5")
wheel cylinder 	1 x 28,57 (1.125") dia.
lining material 	Ferodo primary - 2601 F (thin)
secondary - 2636F (thick)

REAR	S75 P.S.V.
make 	Lockheed
type 	duo-servo drum - auto. adjust
size 	330 x 140 (13" x 5.5")
wheel cylinder 	28,57 (1.25") dia.
lining material 	Ferodo primary (thin) AM 1
secondary (thick) AM 14
lining length 	primary 316 secondary 360

PARKING BRAKE
make 	Clayton Dewandre
type 	spring - pull type
bore 	159 (6.25")
stroke 	50 (1.97")

COLOUR CODING - AIR.PIPES
blue 	split service
yellow 	split service
orange 	parking brake circuit