BRAKES	CHASSIS No. 219001
Data
PRESSURE SETTINGS governor valve - cut in 
- cut out 
safety valve 
quadruple protection valve (all ports) 
hand control valve 
low pressure switch 
parking brake warning switch 	delay valve 

LOAD SENSING VALVE
make 	Lockheed
ratio 	3.3:1
spring colour 	red and blue

NOTE: No L.S.V. on S75 P.S.V.

BRAKE FLUID 	Lockheed Universal 329S (DOT 3 FMVSS 116)
bar	lbf ins2	
8,46 min	123	
9,36/9,64	136/140	
10,34/11,03	150/160	
6,2/6.5	90/94	
6,5/6,2	94/90	
5,2/4,8	75/70	
5,38/5,72	78/83	
12,4	180