BRAKES	CHASSIS No. 219001

AIR/HYDRAULIC

COMPRESSOR
make 	Wabco/Clayton Dewandre
type 	single cylinder - water cooled
capacity 	159cc (7 cu. ft.)

RESERVOIRS
sensing 	1 x 10 litres
service 	2 x 10 litres

ACTUATOR S75 Haulage
make 	Clayton Dewandre
type 	24/24 double diaphragm

ACTUATOR S75 P.S.V.
make 	Clayton Dewandre
type 	475 tandem

MASTER CYLINDER S75 Haulage
make 	Clayton Dewandre
type 	tandem, with integral reservoir and fluid level indicator
diameter 	44,5mm (1.75")
stroke 	50,8mm (2.0")

MASTER CYLINDER	S75 P.S.V.
make 	Clayton Dewandre
type 	tandem with twin independent reservoirs and fluid level indicators
diameter  	44,5	(1.75")	
stroke  	50,8	(2.0")	

BRAKES S75 Haulage
Front
make 	Lockheed
type 	2 leading shoe drum - auto. adjust
size 	300 x 102 (13" x 4")
wheel cylinder 	2 x 31,75 (1.25") dia.
lining material 	Ferodo 263q